**Pope County Fair Pull**

**Saturday August 6th, 2022 Glenwood, MN**

**Start time 3 p.m. Registration starts at 12 p.m. ends at 2:45 p.m.**

**$20/hook Puller’s Pit Pass included additional pit pass $10 must be 12 or older**

**Antique Out of the Field Trucks 3500 (3mph) 9500 (4mph) Factory Gas 6500**

**4000 (3mph) 10500 (4mph) Open Gas 6500**

**4500 (3mph) 11500 (4mph) Factory Diesel 8500**

**5000 (3mph) 12500 (4mph) Improved Diesel 8500**

**5500 (3mph) 15000 (4mph) Open Diesel**

**5500 (5mph) 17500 (4mph) Semis**

**5500 Open 20000 (4mph)**

**6000 (3mph)**

**6000 (5mph) Farm Stock**

**6500 (3mph) 9500 (8mph)**

**6500 (5mph) 10500 (8mph)**

**6500 Open 11500 (8mph)**

**7000 (5mph) 12500 (8mph)**

**7500 (3mph) 12500 Open Jackpot $50 Hook**

**7500 (5mph) 15000 (8mph)**

**7500 Open 17500 Open Jackpot $50 Hook**

**8500 (5mph) Exhibition**

**General Rules Tractor – All decisions and rulings made by the official’s are FINAL.**

* **Max height 20” from ground to top of hook point**
* **Minimum 18” back from center of axle to hook point, no weights on drawbar itself,**
* **100 lbs allowed for weight**
* **Must reweigh before each pull**
* **Only 3 hooks per tractor, you and or tractor cannot pull twice in the same class**
* **Lose anything off the tractor when pulling you will be disqualified**
* **Radial tires are allowed**
* **2 Horns, 2nd horn you’re out**

**Antique- 3 and 5 mph classes, no duals, no turbos, tires size restrictions (see tire chart on back), 40 years and older. 5500, 6500, 7500 Open: no tire restriction or no speed limit.**

**Out of Field- 4 mph, one turbo only, no tire size restrictions, front wheel assist is allowed, duals are allowed.**

**Farm Stock- one turbo only, 8 mph speed limit****, no tire size restrictions, front wheel assist is allowed, duals are allowed.**

**Open Jackpot: $50 entry, Make weight and pull. 1st place takes 50% 2nd takes 25%.**

**Trucks-General Rules-**

* **You must be 16 years old or older and have a valid driver’s license.**
* **Hooking point must not exceed 26” from the top of pulling point to the ground.**
* **Must provide you own clevis or ring hitch to allow a large hook to fit without issue.**

**Factory stock gas 6500 - street legal with current year registration, limit 3 mods**

**Open gas 6500 – open class unlimited mods.**

**Factory diesel 8500 - street legal with current year registration, limit 3 mods (no spool delay and no front weights, no traction bars)**

**Improved diesel 8500 - open class no front weights and must be able to drive on the road legally and have current year registration**

**Open Diesel – open class unlimited mods.**

**Semis- must be street legal and have current year registration.**

**Antique Class Tire Size Chart:**

1. **3,500 lbs**: Tire size: 200 sq. inch  **NO DUALS**
2. **4,000 lbs**: Tire size: 200 sq. inch  **NO DUALS**
3. **4,500 lbs:** Tire size: 200 sq. inch  **NO DUALS**
4. **5,000 lbs**: Tire size: 229 sq. inch **NO DUALS**
5. **5,500 lbs:** Tire size: 229 sq. inch **NO DUALS**
6. **6,000 lbs:** Tire size: 229 sq. inch **NO DUALS**
7. **6,500 lbs**: Tire size: 229 sq. inch **NO DUALS**
8. **7,000 lbs:** Tire size: 300 sq. inch **NO DUALS**
9. **7,500 lbs**: Tire size: 300 sq. inch **NO DUALS**
10. **8,500 lbs:** Tire size: 300 sq. inch **NO DUALS**

**11.2 x 36 = 115 sq. in. 13.6 x 38 = 168 sq. in. 16.9 x 38 = 252 sq. in. 11.2 x 38 = 120 sq. in. 14.9 x 26 = 144 sq. in. 18.4 x 28 = 250 sq. in.**

**12.4 x 36 = 135 sq. in. 14.9 x 28 = 170 sq. in. 18.4 x 34 = 284 sq. in.**

**12.4 x 38 = 140 sq. in. 14.9 x 38 = 200 sq. in. 18.4 x 38 = 300 sq. in.**

**13.6 x 24 = 130 sq. in. 15.5 x 38 = 189 sq. in.**

**13.6 x 28 = 145 sq. in. 16.9 x 34 = 229 sq. in.**

**Austin Pooch (320)-424-1483**

**DuWayne Douvier (320)-424-1240 (leave a message or nobody will get back to you)**